***Non-Mechanical Image Rotation Using an AODP (Acousto-Optic Dove Prism)***

***Eung Gi Paek***

*National Institute of Standards and Technology, Gaithersburg, MD 20899*

***Joon Y. Choe and Tae K. Oh***

*NSWC Dahlgren Division, 17320 Dahlgren , VA 22448-5100*

***John H. Hong and Tallis Y. Chang***

*Rockwell International Science Center, Thousand Oaks, CA 91360*

*Abstract* ***-*** *We report what we believe to be the first method for non-mechanical and programmable image rotation. The method uses a pair of crossed acousto-optic beam deflectors and a polygon mirror to emulate the mechanical dove prism. It is capable of fast (on the order of microseconds) image rotation to an arbitrary angle in a programmable manner. An experimental result to prove the concept is provided.*

Submitted to Optics Letters on April 15, 1997

Rotation of an image to an arbPeer Reviewed PublicationsFrom MMS Environmental Studies1999 – 2003Aaron, T., D.K. Mellinger, and A. Martinez. 2002. Passive three-dimensional tracking of sperm whales using two towed arrays during the 2001 SWAMP cruise. The Journal of the Acoustical Society of America. November 2002, 112(5):2399.Abookire, A. A.; Piatt, J. F., and Norcross, B. L. Juvenile groundfish habitat in Kachemak Bay, Alaska, during late summer. Alaska Fishery Research Bulletin 8. 2001:45-56.Ambrose, R.F., Lee, S.F., and S. Bergquist. 2002. Sediment disposal site rocky intertidal monitoring studies:  Santa Monica to Malibu Coastline. Report to the State of California Department of Transportation District 7. (With Addendum: Data and Field Notes.)Amstrup, S.C.; Weston-York, G.; McDonald, T.L.; Nielson, R.; Simac, K. 2003. Detecting denning polar bears with Forward Looking Infra-red Imagery (FLIR). USGS Science Center. BioScience March 4, 2003.Ata, A., Kerr, R.G., Moya, C.E., and R.S. Jacobs.(in press). Identification of anti-inflammatory diterpenes from the marine gorgonian Pseudopterogorgia elisabethae. Tetrahedron Beckenbach, E.H., Washburn, L., Salazar, D., and B. Emery. 2000. Observations of Propagating Eddies in the Santa Barbara Channel. EOS Trans.Amer. Geophys.Union 81 (48): Fall Meet. Suppl. Becker. P.R.; Krahn, M. M.; Mackey, A.; Demiralp, R.; Schantz, M. M.; Epstein, M.; Donais, M. K.; Porter, B.; Muir, C. G., and Wise, S. A. Concentrations of Polychorinated Biphenyls (PCBs), Chlorinated Pesticides, and Heavy Metals and Other Elements in Tissues of Beluga Whales (Delphinapterus Leucas) From Cook Inlet, Alaska. Marine Fisheries Review. 2000 (62):81-98.Boles, J.R., J.F. Clark, I. Leifer, and L. Washburn. 2001. Temporal variation in natural methane seep rate due to tides, Coal Oil Point area, California. J. Geophys. Res. 106(C11):27077-27086.Byrnes, M.R., R.M. Hammer, T.D. Thibaut (in press). Potential physical and biological effects of sand mining off New Jersey. Journal of Coastal Research, Special Issue.Byrnes, M.R., R.M. Hammer, T.D. Thibaut (in press). Potential physical and biological effects of sand mining off Alabama. Journal of Coastal Research, Special Issue.Candela, J., J. Sheinbaum, J. Ochoa, A. Bedan and R. Leben. 2002. The potential vorticity flux through the Yucatan Channel and the Loop Current in the Gulf of Mexico. Geophys. Res. Lett. 29:16-1 to 16-4.Chen, C-S., and D-P. Wang, 2000. Data assimilation model study of wind effects in the Santa Barbara Channel, J.Geophys. Res., 105 (C9):22,003-22,013Christopher, S. J.; Vander Pol, S. S.; Pugh, R. S.; Day, R. D., and Becker, P. R. 2002. Determination of mercury in the eggs of common murres (Uria aalge) for the seabird tissue archival and monitoring project. The Royal Society of Chemistry 2002. 2002:17Clark, J.F., L. Washburn, J.S. Hornafius, and B.P. Luyendyk. 2000. Dissolved hydrocarbon flux from natural marine seeps to the southern California Bight. J of Geophys Res-Oceans 105 (C5):11509-11522.Continental Shelf Associates. 2002. Survey of Invertebrate and Algal Communities on Oil and Gas Platforms in Southern California. Final Report in Press. U.S. Department of the Interior, Minerals Management Service, Pacific OCS Region. 102 pp.+ 5 appendices.Davis, R. W., J.G. Ortega-Ortiz, C.A. Ribic, W.E. Evans, D.C. Biggs, P.H. Ressler, R.B. Cady, R.R. Leben, K.D. Mullin and B. Wursig. 2002. Cetacean habitat in the northern oceanic Gulf of Mexico. Deep-Sea Research Part I-Oceanographic Research Paper. 49 (1):121-142.Deacon, R. T. and C. D. Kolstad. 2000. Valuing Beach Recreation Lost in Environmental Accidents. J. Water Resources Planning & Mgmt 126:374-81.De Leeuw, G. and I. Leifer. 2001. Bubbles outside the bubble plume during the LUMINY wind-wave experiment. In Gas Transfer and Water Surfaces, Eds. M. Donelan, W. Drennan, E.S. Salzman, and R. Wanninkhof. AGU Monograph 127:295-301.Dever, E.P. 2002. Objective maps of near-surface flow states near Pt. Conception, California. J. Phys. Oceanography Dever, E.P., and C.D. Winant, 2002. The evolution and depth structure of shelf and slope temperatures and velocities during the 1997-1998 El Nino near Point Conception, California, Progress in Oceanography 54:77-103Diaz, R. J., G. R. Cutter, Jr. and K. W. Able. 2003. The importance of physical and biogenic structure to juvenile fishes on the shallow inner continental shelf. Estuaries 26:12-20. Diaz, Robert, J.P. Maa, and C.H. Hobbs, III (in press). Possible impacts of sand mining offshore of Maryland and Delaware: Part 2 – on Biological Aspects. Journal of Coastal Research.Dorman, C. E., and C. D. Winant, 2000. The structure and variability of the marine atmosphere around the Santa Barbara Channel, Mon. Weather Review 128(2):261-282. Duesterloh, S.; Short, J. W., and Barron, M. G. 2002. Photoenhanced Toxicity of Weathered Alaska North Slope Crude Oil to the Calanoid Copepods Calanus marshallae and Metridia okhotensis. Enivironmental Science and Technology 36(18):3953-3959.Dugan, J. E., D.M. Hubbard and M. Lastra. 2000. Burrowing abilities and swash behavior of three crabs, Emerita analoga Stimpson, Blepharipoda occidentalis Randall, and Lepidopa californica Efford  (Anomura, Hippoidea), of exposed sandy beaches.  J. Exp. Mar. Biol. Ecol. 255(2):229-245.Dugan, J. E., D.M. Hubbard, J.M. Engle, D.L. Martin, D.M. Richards, G.E. Davis, K.D. Lafferty, and R.F. Ambrose. 2000. Macrofauna communities of exposed sandy beaches on the Southern California mainland and Channel Islands. Fifth California Islands Symposium, pp 339-346.  Dugan, J.E., Hubbard, D.M., McCrary, M., and M. Pierson (in press). The response of macrofauna communities and shorebirds to macrophyte wrack subsidies on exposed sandy beaches of southern California. Estuar. Coastl. Shelf Sci. Durner, G. M. Amstrup S. C. McDonald T. L. 2001. Estimating the impacts of oil spills on polar bears. Arctic Research of the United States. 2001; 14 (Fall/Winter):33-37.Emery, B.M., L. Washburn, and J. Harlan.(in press). Evaluating CODAR high frequency radars for measuring surface currents: observations in the Santa Barbara Channel, Journal of Atmospheric and Oceanic Technology Ezer, T. and L.Y. Oey. 2002. Modes of variability in the Yucatan Channel Flow, EOS Trans. Supplement, Amer. Geophys. Union, 83(47):712.Ezer, T., L.Y. Oey. and H.C. Lee. 2002. Simulation of velocities in the Yucatan Channel, In: Proc., Oceans 2002. Published by MTS/IEEE: 1467-1471.Flegal, A.R., I. Rivera-Duarte, and S. Sañudo-Wilhelmy (in press). Silver contamination in aquatic environments. Review in Environmental Chemistry and Toxicology. Forde, S.E. 2002. Modelling the effects of an oil spill on open populations of intertidal invertebrates. Journal of Applied Ecology 39:595-604.Gaylord, B., Reed, D.C., Raimondi, P.T., Washburn, L., and McLean, S.R. 2001. A physically based model of macroalgal spore dispersal in the wave and current dominated nearshore. Ecology 83: 1239-1251 Gonzalez-Guzman, L., S. Gaines, and J. Dugan. 2001. Environmental suitability across the geographic distribution of marine intertidal invertebrates. Bull. Ecol. Soc. Amer. 82.Hamdoun, A.M., Griffin, F.J., and G.N. Cherr. 2002. Tolerance to biodegraded crude oil in marine invertebrate embryos and larvae is associated with expression of a multixenobiotic resistance transporter. Aquat. Toxicol. 61(1-2):127-140. Hamilton, P., T.J. Berger, and W. Johnson. (in press). On the structure and motions of cyclones in the northern Gulf of Mexico. J. Geophys. Res. Harding, Ann M. A.; van Pelt, Thomas I.; Piatt, John F., and Kitaysky, Alexander S. 2002. Reduction of Provisioning Effort in Response to Experimental Manipulatiitrary angle in a programmable manner is very important for various applications such as rotational invariant pattern recognition, computer graphics and beam steering of phased array antennas.

Most of the previous techniques [1-5] rely on a dove prism as shown in Figure 1 (a). By rotating a dove prism by an angle  around the optical axis, an input image can be rotated by 2. However, such a mechanical process is slow and unreliable. Chiou and Yeh [6] demonstrated a non-mechanical method using a conventional dove prism inside a ring cavity to generate a series of rotated images.

In this Letter, we propose an image rotation method that is both non-mechanical and programmable to permit rotation of an image to an arbitrary angle in a controllable manner. It is based on an analysis of a conventional dove prism. As illustrated in Figure 1 (b), a dove prism can be divided into three parts: the first part is a wedge prism to direct the incident beam to the bottom (or top) of the second part which functions as a mirror to reflect the incoming light. The third part is another wedge prism to redirect the beam along the original direction. All these three parts rotate together.

Our approach for non-mechanical image rotation is shown in Figure 1 (c). Each of the rotating wedges (the first and third parts of a dove prism) is replaced by an xy acousto-optic beam deflector (xy-AOBD). The xy-AOBD consists of a pair of crossed AOBD’s sandwiched together with transducers along orthogonal directions. Byadjusting the frequencies of acoustic signals applied to the two AOBD’s, beam direction can be changed along arbitrary directions, just as a wedge does.

The reflecting mirror (second part) is replaced by a circular cylindrical mirror to avoid the need for rotation. However, to prevent unwanted distortion due to the curvature of the circular mirror surface, the cylindrical mirror is discretized to multiple facets. Also, incoming light is focused to have a minimum size on the mirror surface. In this way, an image can be rotated fast (on the order of microseconds) to an arbitrary angle in a programmable manner, without requiring any moving parts. Since the concept is based on the conventional dove prism, a name acousto-optic dove prism (AODP) has been proposed.

To prove the concept of the proposed AODP, we constructed an experimental setup as shown in Figure 2. A 5 mW HeNe laser is used as the light source. After beam expansion and spatial filtering, the magnified collimated beam illuminates an input resolution target. The light passing through the input transparency is deflected by a pair of crossed AOBDs (slow shear mode TeO2 crystals with a large input angular bandwidth) and is focused by a lens (focal length = 36 cm) on the surface of the cylindrical polygon mirror. In this initial demo intended for proof of our concept, only two mirror facets oriented at a right angle are used. After the multi-facet mirror, the beam is reflected back to pass through the same lens and xy-AOBDs and is detected by a CCD after a beam splitter.

Figure 3 illustrates an experimental result obtained from our optical system. Since the two mirrors are at a right angle, the two images are rotated by 180 degrees (twice the angle between the two mirrors). A real-time image rotation has been achieved within 10 sec with a 6 mm aperture in front of the AOBDs. Also, rotations to other angles have been separately confirmed.

The noise contribution to the image is mainly due to unwanted reflection from the surfaces of optical components such as the beam splitter, AOBDs and the lens. Also, a slight defocusing of the images is attributed to the distance between the two AOBDs. These noises can be greatly reduced if thin sandwiched xy-AOBD’s (shown in Figure 1 (c)) are used. A custom-designed xy-AOBD with a compact size (10 mm X 10mm X 2mm) and with xy transducers on the same crystal is currently being fabricated.

The number of different rotation angles available in this system is given by the following equation:

, (1)

where f, dmin and v represent acoustic frequency bandwidth, minimum feature size of an input pattern and acoustic velocity, respectively. Interestingly, the number is independent of the focal length of a lens and wavelength of the light. For a typical example, f = 50 MHz, dmin = 0.1 mm and v = 600 m/sec, N becomes approximately 25.

To further increase the number of rotation angles, several methods can be used: First, a special lens design can be employed to reduce the fixed distortion effect of a cylindrical mirror. Second, higher-order diffracted beams can be used instead of the first order to increase the diffraction angle of an AOBD. In this case, the thickness of an AOBD needs to be thin to reduce the Q factor [7] and to permit higher-order diffractions. Taking the third order diffraction, for example, would permit rotation to 75 different angles, which is normally sufficient for rotationally invariant pattern recognition. In this case, other unwanted diffraction orders can be discarded simply by choosing the appropriate length of the cylindrical polygon mirror.

The AOBDs in this system need to accept an input beam with broad angular bandwidth of approximately 3 degrees. A special group of AOBDs (typically, slow shear wave Tellurium dioxide crystals) that accept a circular laser beam are commercially available.

In conclusion, we have proposed and demonstrated what we believe to be the first non-mechanical image rotation method that can be programmed to permit rotation of an image to an arbitrary angle within a few microseconds time. The method can be useful for various information processing applications such as rotationally invariant pattern recognition and computer graphics.

This work was supported by the Office of Naval Research (ONR) under Contract Number NC0014-97-F-0021.

**References**

R. B. Johnson, Appl. Opt. 13, 2962 (1974), US Patent 3,813,552.

W.G. McKinley, Appl. Opt. 33, (28) 6570 (1994), US Patent 5,296,972.

R.H. Ginsberg, Appl. Opt. 33, (34) 8105 (1994).

B. Braunecker, O. Bryngdahl, and B. Schnell, J. Opt. Soc. Am. 70, 137 (1980).

A. W. Lohmann, J. Opt. Soc. Am. A 10, 2181 (1993).

A. Chiou, and Pochi Yeh, Apl. Opt. 29, 1584 (1990).

R.J. Collier, C.B. Burckhardt and L.H. Lin, *Optical Holography* (Academic Press, New York, 1971), Chap. 9.

**Figure Captions:**

Figure 1. Image rotation methods : (a) conventional mechanical method using a dove prism, (b) three parts of a dove prism and (c) the proposed non-mechanical image rotation using an AODP (acousto-optic dove prism).

Figure 2. Experimental setup. Two orthogonal mirrors are used as a polygon mirror in this proof-of-concept experiment.

Figure 3. Experimental results of non-mechanical image rotation. The rotation angle of the two images and (a) and (b) is 180 degrees which is twice the angle between the two mirror facets at a right angle.